{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Directions","UK TAG","Sheet1","zRef_Drop_Downs","MonRoundInfo"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Directions","index":0,"n_rows":21,"n_cols":3,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"These Guidelines have been transposed from the original at: "]
[null,null,"http://www.wfduk.org/sites/default/files/Media/UKTAG_Technical%20report_GW_Haz-Subs_ForWebfinal.pdf"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Disclaimer: All care has been exercised in the compilation of these guidelines for quick import to ESDAT, \nhowever no liability is taken for any error.  It is the responsibility of the user to review the contained data \nand ensure their data is compliant with the relevant guidelines, and that this compilation meets their requirements.  "]

{"sheet":"UK TAG","index":1,"n_rows":59,"n_cols":28,"rows_kept":59,"cut":false,"hidden":false,"merged":[]}
["Project:",null,null,"Table:","[zRef_Environmental_Standards]",null,"Style:","Template","HasLocs"]
["ODBC:",null,null,"Parent Tables:","zRef_Matrix_Types,zRef_Chemistry_Lookup",null,"OnlineBaseURL:","https://online-usa.esdat.net"]
[]
["ChemCode","ChemName","MatrixType","ActionLevelSource","ActionLevel","ActionLevel_Min","Units","Leached","Comments","ActionLevel_Prefix","ActionLevel_Suffix","Conditional_Matrix_Type","Conditional_Depth_From","Conditional_Depth_To","Conditional_ChemCode1","Conditional_ChemCode1_Units","Conditional_ChemCode1_Value_Min","Conditional_ChemCode1_Min_Value_Prefix","Conditional_ChemCode1_Value_Max","Conditional_ChemCode1_Max_Value_Prefix","Conditional_ChemCode2","Conditional_ChemCode2_Units","Conditional_ChemCode2_Value_Min","Conditional_ChemCode2_Min_Value_Prefix","Conditional_ChemCode2_Value_Max","Conditional_ChemCode2_Max_Value_Prefix","Applies_To_Total_Result","Applies_To_Filtered_Result"]
["79-06-1","Acrylamide","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["85535-84-8","Alkanes, C10–13, chloro","Water","UKTAG values for hazardous substances",105,null,"ug/L"]
["120-12-7","Anthracene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["7440-38-2","Arsenic","Water","UKTAG values for hazardous substances",5,null,"ug/L"]
["71-43-2","Benzene","Water","UKTAG values for hazardous substances",0.5,null,"ug/L"]
["50-32-8","Benzo(a)pyrene","Water","UKTAG values for hazardous substances",5.0000000000000001E-3,null,"ug/L"]
["205-99-2","Benzo(b)fluoroanthene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["191-24-2","Benzo(g,h,i)perylene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["207-08-9","Benzo(k)fluoranthene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["75-01-4","Chloroethylene / (Vinyl\r\nChloride)","Water","UKTAG values for hazardous substances",0.25,null,"ug/L"]
["18540-29-9","Chromium(VI)","Water","UKTAG values for hazardous substances",5,null,"ug/L"]
["Dioxins","Dioxins","Water","UKTAG values for hazardous substances",1.5E-5,null,"ug/L"]
["25637-99-4","Hexabromocyclododecane\r\n(HBCDD)","Water","UKTAG values for hazardous substances",350,null,"ug/L"]
["118-74-1","Hexachlorobenzene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["87-68-3","Hexachlorobutadiene (HCBD)","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["58-89-9","Hexachlorocyclohexane","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["193-39-5","Indeno(1,2,3-cd)pyrene","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["7439-92-1","Lead","Water","UKTAG values for hazardous substances",5,null,"ug/L"]
["7487-94-7","Mercury compounds","Water","UKTAG values for hazardous substances",0.5,null,"ug/L"]
["1763-23-1","Perfluorooctane sulfonic acid and its salts (PFOS)","Water","UKTAG values for hazardous substances",1,null,"ug/L"]
["608-93-5","Pentachlorobenzene","Water","UKTAG values for hazardous substances",2,null,"ug/L"]
["56-35-9","Tributyltin oxide (TBTO)","Water","UKTAG values for hazardous substances",1,null,"ug/L"]
["79-01-6","Trichloroethylene","Water","UKTAG values for hazardous substances",5,null,"ug/L"]
["120-82-1","1,2,4-trichlorobenzene","Water","UKTAG values for hazardous substances",35,null,"ug/L"]
["120-83-2","2,4-dichlorophenol","Water","UKTAG values for hazardous substances",100,null,"ug/L"]
["95-57-8","2-chlorophenol","Water","UKTAG values for hazardous substances",150,null,"ug/L"]
["59-50-7","4-chloro-3-methylphenol","Water","UKTAG values for hazardous substances",350,null,"ug/L"]
["309-00-2","Aldrin","Water","UKTAG values for hazardous substances",1.4999999999999999E-2,null,"ug/L"]
["1912-24-9","Atrazine","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["2642-71-9","Azinphos ethyl","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["86-50-0","Azinphos methyl","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["56-23-5","Carbon tetrachloride","Water","UKTAG values for hazardous substances",1.5,null,"ug/L"]
["470-90-6","Chlorfenvinphos","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["67-66-3","Chloroform","Water","UKTAG values for hazardous substances",50,null,"ug/L"]
["50-29-3","DDT","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["17040-19-6","Demeton-S-methyl sulphone","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["333-41-5","Diazinon","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["60-57-1","Dieldrin","Water","UKTAG values for hazardous substances",1.4999999999999999E-2,null,"ug/L"]
["60-51-5","Dimethoate","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["115-29-7","Endosulfan","Water","UKTAG values for hazardous substances",10,null,"ug/L"]
["72-20-8","Endrin","Water","UKTAG values for hazardous substances",1.4999999999999999E-2,null,"ug/L"]
["122-14-5","Fenitrothion","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["55-38-9","Fenthion","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["465-73-6","Isodrin","Water","UKTAG values for hazardous substances",1.4999999999999999E-2,null,"ug/L"]
["121-75-5","Malathion","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["7786-34-7","Mevinphos","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["56-38-2","Parathion","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["298-00-0","Parathion-methyl","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["1336-36-4","PCBs","Water","UKTAG values for hazardous substances",0.25,null,"ug/L"]
["87-86-5","Pentachlorophenol (PCP)","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["52645-53-1","Permethrin","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["122-34-9","Simazine","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["108-88-3","Toluene","Water","UKTAG values for hazardous substances",350,null,"ug/L"]
["1582-09-8","Trifluralin","Water","UKTAG values for hazardous substances",0.05,null,"ug/L"]
["76-87-9","Triphenyltin oxide (TPTO)","Water","UKTAG values for hazardous substances",1,null,"ug/L"]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"zRef_Drop_Downs","index":3,"n_rows":1,"n_cols":3,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["Table","Column","Values"]

{"sheet":"MonRoundInfo","index":4,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":true,"merged":[]}
["Monitoring_Round"]
["Project_ID"]
["PID"]